VXD3: NEW VERTEX DETECTOR

• Increased polar angle coverage ⇒ cos θ ∼ 0.72 → 0.85

• Better ϕ coverage

⇒ ∼2.3 increases to ∼3.2 hits/track

• Less material

⇒ L/LR/Layer decreases from 1.1% to 0.5%

• Increased lever arm

⇒ From 1.2 cm to 1.99 cm

VXD3/VXD2 COMPARISONS